[bookmark: _GoBack]INTERIOR FUSEBOX (located under the glove box, its the panel with a hole in it and just pulls off)
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ENGINE FUSEBOX (located at the far right of the engine bay and simply unclips and lifts)
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Fuse box : 13 fuses under the dashboard.

Rating Functions
5A | ABS (warning lamp) - Coolant temperature control unit - Tachometer - Diesel prehealing -
or 25 A* | Diagnostic socket - Automatic gearbox (relay) - Air conditioning cutoff relay - Electric
shul-off - Warning lamps and gauges
25 A | Rear view mirror demister control - Air conditioning blower - Heated rear screen - Power-
assisted steering
25A | Unused
90 A | Lights-on audible warning - Direction indicators - Electric window - Clock - Radio - Day-
fime lamps. - Eleclric rear view mirror - Charge warning lamp
30A | Cigar lighter - Horn - Healed rear screen - Demisting rear view mirror
10 A | Hazard warning lamps
45 A | Stop lamps switch - Reversing lamp - Automatic gearbox (ecu)
20 A | Central locking - Boot lighting - Interior lighting - Clock memory - Radio memory - Remote
control - Diagnostic socket - Coolant temperature control unit
20 A | Windscreen/rearscreen wipers - Windscreen washer - Windscreen wipe timer - Map
or 30 A* | reading lamp - Sun roof
80 A | Electric window
5A | Foglamp
5A | Audio system - Lightson audible warning - Daytime lamps control - Fagade lighting -
Lighting with rheostat/without rheostat - Front right, front left, rear right sidelamps - Air
conditioning switch - Sidelamp warning lamp - Cigar lighter
5A | Number plate lighting - Rear left sidelamp
5A | Heated seats
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Numb.r: Functions
F1 15 A Injection ECU
= 30A |naBs
Tra 30A [ cooling fan unit
Fa 30A |ass
Fs 30A | Gooling fan unit
15A | Foglamp
20 A Daytime lamps
Z 20 A | Headlamp washer
10A | Fuel pump
20A | Automatic gearbox - Pre-post heating - Double injection relay - ABS (warning lamp) -
Coolant temperature control unit
5A Oxygen sensor (catalytic converter)
E12 10 A Left hand main beam
F13 [ 10A [Right hand main beam
_F1a 10A | Left dipped beam - Headiamp wash timer
F15 10 A Right dipped beam
Single 30A [ Air pump (control)





