Hi,

has anybody installed CF in an Opel and uses OBD-II?
I have a lot of different interfaces but no one works...
ELM320, 322 and 323 says nothing...
When i connect my ELM 327, CF says connected, but i see no engine data...0

Does Opel use a special kind of protocol?
Mine works find on a 07 Vectra C......

Terran
Which one? ELM327? Which parameters (bits per second, pairity, flowcontrol...) did you use?

My car is a 03 Astra G.
I use 9600-8-N-1-N
ELM327 1.2a - 9600 and default settings I think.

Terran
You need to narrow the problem down a little bit.
Try this:

1. power off and then power on the scantool
2. Start hyperterminal and set parameters to 9600 N81 and type in ATI
3. You should see a response like 'ELM327 ...'
4. Then just type 0100 and see what the response is

If you don't get that far, then something is wrong. I don't know what CF looks for before showing 'connected',but from reading other posts I think it has to do with the ATI response which describes the scantool in use... 

What responses do you get using the method above?
When typing ATI it posts "ELM327 v1.0a"
When typing 0100 it posts "UNABLE TO CONNECT"
Ok, well you're connected to the scantool, but the scantool isn't connected to the car. This isn't a CF problem.

What scantool are you using and what model and year is your car?
Thsi scantool: more info obd2

The car is from 2003

I found in some forums that cars from Opel didnÂ´t use OBDII. Only KWP200... Can that be?
ISO14230 (KWP2000) is a protocol for OBD-II - there are a number of protocols that your car can use, yours just happens to use KWP2000. The scantool you linked to says it supports that protocol so it should work.

You do have the engine running when your trying to read date aren't you?

Another possibility is that the scantool is set to the wrong protocol. The scantools can be set to either try each protocol every time it's connected until it finds the right one, trys a preferred protocol before trying the rest or is set to one protocol only which is what may have happened.

Try
1. power off and then power on the scantool
2. Start hyperterminal and set parameters to 9600 N81 and type in ATSP4.
3. power off and then power on the scantool

If that doesn't work, try using ATSP5.

ATSP4 and ATSP5 will set the protocol of the scantool to either of the KWP protocols.
After step 3 i tried to type 0100.
It says BUS INIT....ERROR

I think it really didnÂ´t work with my Opel :-(
Try using ATSP5.

The bus init...error message is a wrong protocol message.
I tried both...
Did you have a list with all protocols? Than i could try all....
0 - Automatic
1 - SAE J1850 PWM (41.6 Kbaud)
2 - SAE J1850 VPW (10.4 Kbaud)
3 - ISO 9141-2 (5 baud init, 10.4 Kbaud)
4 - ISO 14230-4 KWP (5 baud init, 10.4Kbaud)
5 - ISO 14230-4 KWP (fast init, 10.4 Kbaud)
6 - ISO 15765-4 CAN (11 bit ID, 500 Kbaud)
7 - ISO 15765-4 CAN (29 bit ID, 500 Kbaud)
8 - ISO 15765-4 CAN (11 bit ID, 250 Kbaud)
9 - ISO 15765-4 CAN (29 bit ID, 250 Kbaud)

The Automatic selection (protocol 0) instructs OBDPro to try all protocols, when looking for a valid one. It will first try protocol 1, then will sequence through each of the others, until the correct one used by the vehicle is identified.If a non zero protocol is selected with this command (eg. ATSP 3), that protocol will become the default. Failure to initiate a connection in this situation will result in responses such as BUS INIT: ...ERROR. If you know the protocol used by your vehicle; setting the protocol manually saves time in trying to detect the protocol.

Shamelessly copied from OBDPros
hello,

has anyone managed talking to the Opel Astra G 2003?
could you please post an example??
I know that many of the modules of AstraG, like airbag or aircon, use KW82 protocol which is not supported by elm327.

Thanks
you will never getting it running bequase opel is using tech2.
you can buy a opcom and get the data, but it isn't gone work with centrafuse.
Sorry for my bad english

you need for your opel 

tech2 interface without CANBUS 

or

OPCOM interface(multiplexer) wenn your car have CanBUS

my Opel Vivaro Diesel Year 2004 dont work with ELM or AGV interfaces

i became a interface on ebay from CHINA or Britan

follow this ebay number
250771305986

greeting from Germany
yer corsa's and astra's and zafira's it works for up to now and for people who dont know how do the "pedal trick" 

No need for Tech 2 or any sort of code readers and Most of Vauxhall dealers don’t know about this....

When you get into the car you know the key has 3 clicks first on for aftermarket cd player and whatever else and the second one the dash comes on third the starter kicks in 

before you put the key into the ignition Make sure that you Press the Break and the Throttle to the Floor ( max )
Then turn the key on until The dash board come on and DONT START THE CAR 
Wait 2 sec and keep the pedals Down to the floor 
the service light under the management light should start flashing 

it will flash 4 times leaving 2 second space representing each number 
Zero gets 10 flashes 

for exampleP0110
the light will flash ten times Break (2sec Or 1 not sure) then once, (2sec) once again, then ten

if you have more than one code it will stop for a break then gives the next code 

however if you don’t have any code stored it will start Flashing and keeps on flashing until you release the paddles 

so i have done the pedal trick andit just keeps flashin constently until i release the pedals, what could be my problem be now, i still have all the symptoms of a computer failure, hesitant off the mark, can't go over 80m.p.h because when i come off onto the slip road and press the brake the engine just cuts out, i have grey slime on the cap of my oil re-fill cap. but no symptoms of a gasket gone other than that one? any ideas????????????
NO NO NO ,,, if the light keeps flashing means no codes are stored or pending , your car's symptoms are more like EGR valve which will not necessarily trigger a fault code , clean it or replace it ,
the grey slime is just common to 8v build up condensation inside the engine combined with short cold journeys
This is very useful information. Thanks. 

I just came from the mechanic and his system was showing following codes as undocumented code. I have a problem that my dual fuel car is not giving power on 4th and 5th gear on Petrol. It is running fine on LPG. I have this problem from quiet sometime and hence using care only on LPG. I have driven around 5K miles on LPG without any major problem but the problem on Petrol still exists. Two local mechanic told me that ECU needs to be replaced and cost is very high. Not worth spending on 2002 model old car! Don't know what should I do? Any good suggesstion!
are you pressing the brake and acceleration down to the floor and waiting till all the dash lights glow up then the car with the spanner should light up ?
it should do works for a corsa c and astra mk4 which is same base as the zafira
ukljuciti kontakt i sledi brojanje blinkanja check engine lampice
za označavanje početka i kraja dijagnoze lampica označava broj 12
znači,blinkne jednom pa dvaput = 1+2=12 i tako tri puta za početak dijagnoze
i tri puta za kraj dijagnoze!

na primer: kada lampica blinkne tri puta pa pauza pa jednom to je broj 31 i tako tri puta
za svaku grešku!
znači:31,31,31 je ispis za jednu grešku!

dole je primer tog čitanja(brojanja)
na snimku se vidi znači početak programa (tri puta blinkne broj 12)
i onda sljedi čitanje ostalih eventualnih grešaka koje motor ima ili koje je ECU memorisao u memoriju
na snimku se vidi nakon broja 12 je broj 31(blinkne tri puta pa jednom) i tako tri puta
a označava senzor radilice pošto motor miruje
nakon toga blinka opet broj 12 za kraj programa jer grešaka nema
i taj proces vrti unedogled!
znači:12,12,12...31,31,31...12,12,12...
da motor radi i ako nema grešaka lampica blinka samo broj 12
znači,broji se blinkanje i sabirajaju se brojevi u jedan celi broj!

konektor prespojiti zicom kao na slici:
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konektori:
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ovde mozete detaljno i opsirnije da progledate upustvo sa kodovima i nazivima gresaka za razlicite sisteme kod opela:

http://www.topbuzz.co.uk/info/fault_cod ... _codes.htm

napomena: Belmont = Kadett
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