Abreviaturas ecu Toyota
Abbreviations and Toyota/SAE terms:
Glossary of SAE and Toyota Terms

SAEAbbreviations_______SAETerms_____TOYOTATerms





ACH Air Cleaner Housing Air Cleaner
ACS Air Conditioning Sensor Air Conditioning Switch
AFS Air Flow Sensor Air Flow Meter
AIR Secondary Air Injection Air Injection (AI)
ALT Alternator Alternator
B+ Battery Positive Voltage +B, Battery Voltage
BARO Barametric Absolute Pressure Sensor HAC Sensor or P sensor
CAC Charge Air Cooler Intercooler
CARB CArburetor Carburetor
CL Closed Loop Closed Loop
CLS Closed Loop System Closed Loop System
CPS Crankshaft Position Sensor Crank Angle Sensor
DI Direct Injecttion Direct Injection
DLC1
DLC2 Data Link Connector 1: Check Connector
2: TDCL
DLI Distributerless Ignition Distributerless Ignition
DTC Diagnostic Trouble Codes Diagnostic Codes
ECTS Engine Coolant Temperature Sensor Coolant Temperature Sensor, Water Temperature Sensor or THW
EEPROM Electrically Erasable Programmable Read Only Memory Electrically Erasable Programable Read Only Memory (EEPROM), Erasable Read Only Memory (EPROM)
EFE Early Fuel Evaporation Cold Mixture Heater (CMH), Heat Control Vavle (HCV)
EGR Exhaust Gas Recirculation Exhaust Gas Recirculation
EGRS EGR Function Sensor EGR Gas Temperature Sensor
EGRV EGR Valve EGR Valve
EI Electronic Ignition Electronic Spark Advance (ESA)
EM Engine Modification Engine Modification
EPROM Electrically Programmable Read Only Memory Programable Read Only Memory (PROM)
EVAP Fuel Evaporative System Evaporative Emission Control
FPR Fuel Pump Relay Fuel Pump Relay
GND Ground Ground
HO2S Heated Oxygen Sensor Heated Oxygen Sensor
IACV Idle Air Control Valve ISC Valve
IATS Intake Air Temperaure Sensore Intake or Inlet Air Temperature Sensor
IDI Indirect Diesel Injection Indirect Injection Diesel Engine
KS Knock Sensor Knock Sensor
MAP Manifold Absolute Pressure Sensor Manifold Pressure Sensor
Turbocharger Pressure Sensor
Vacuum Sensor
MCS Mixture Control Solenoid Electric Bleed Air Conrtol Valve (EBCV)
Electric Air Control Valve (EACV)
MPI Multipoint Fuel Injection Electronic Fuel Injection (EFI)
O2S Oxygen Sensor Oxygen Sensor, O2 Sensor
OBD On Board Diagnostic System On-Board Diagnostic System
OC Oxidation Catalyst Oxidation Catalyst, CCo
OL Open Loop Open Loop
PAIR Pulsed Secondary Air Air Suction (AS)
PCME Powertrain Control Module (engine) Engine ECU
PCME&T Powertrain Control Module (engine and transmission) Engine and ECT ECU
PCMT Powertrain Control Module (transmission) ECT-ECU, Transmission ECU
PNS Park/Neutral Switch Neutral Start Switch (NSW)
PTCS Powertrain Control Signals Output Signals
PTIS Powertrain Input Signals Inp[ut Signals
RAM Random Access Memory Random Access Memory
ROM Read Only Memory Read Only Memory
SABFV Secondary Air Anti-Backfire Valve Check Valve
SABV Secondary Air By-Pass Valve Air By-Pass Valve (ABV)
SAPV Secondary Air Pulse Valve AS Reed Valve, Air Suction Valve
SASV Secondary Air Switching Valve Air Switching Valve (ASV)
SC Supercharger Supercharger
SMPI Sequential Multipoint Electronic Fuel Injection Electronic Fuel Injection (EFI), Sequential Injection
SPS Steering Pressure Sensor Air Control Valve (ACV)
TB Throttle Body Throttle Body
TBI Throttle Body Electronic Fuel Injection Single Point Injection
Central Fuel Injection (Ci)
TC Turbocharger Turbocharger
TCC Transmission/Transaxle Converter Clutch Switch Lock-Up Solenoid
TGSS Transmission Gear Selector Switch Shift Possition Switch
TOP Trap Oxidizer-Periodic Diesel Particulate Filter (DPF)
Diesel Particulate Trap (DPT)
TPS Throttle Possition Sensor Throttle Possition Sensor
TVS Thermal Vacuum Switch Bimetal Vacuum Switching Valve (BVSV)
Thermostatic Vacuum Switching Valve
TWC Three Way Catalyst Three Way Catalyst
CC80
VR Voltage Regulator Voltage Regulator
VSPG Vehicle Speed Pulse Generator Speed Sensor
VSS Vehicle Speed Sensor Vehicle Speed Sensor (reed switch type)
WOTS Wide Open Throttle Switch VL Switch
Power Switch
WUTWC Warm Up Three Way Catalyst Manifold Convertor






these may help too



ECU Pinout




E01 Earth 01 Brown
E02 Earth 02 Brown
#1 Injector output Red/White
#2 Injector output White/Blue
#3 Injector output Black/White
#4 Injector output Green/Yellow
RSO Idle air control output Red
RSC Idle air control output Green
HT Oxygen sensor heater output Red/White
STJ Cold start injector output Green
IGT Ignitor signal White
EGR EGR output (optional) Black/Red
G2 Distributer input White
G1 Distributer input Green
NE Distributer input Black
G- Distributer input Red
IGF Ignitor signal White/Red
TPC Turbo presure control output (to turbo VSV) Blue/Orange
TVIS Control Signal to TVIS solenoid Green/Black
E1 Earth 1 Brown
VF Check connector signal (EGO feedback signal) Red/White
TE1 Test signal Orange
TE2 Test signal Black?
OX Oxygen sensor input Black
PIM MAP sensor input Blue/Black
KNK Knock sensor input Black
THW Coolant temperature input Red
IDL Idle switch on throttle position sensor Purple
THA Intake air temperatur input Black
VTA Throttle position input White
VS Airflow sensor input Yellow/Blue
THG EGR function sensor (optional) Black/Yellow
VC 5V ouput for MAP, throttle position and airflow sensors Red/Blue
E2 Ground/earth output for sensors Brown
STA Clutch start switch input (optional?) Red
AC Aircon request input Black/White
SPD Speed sensor input Violet/White
PS Power steering signal Black
PSCT Power steering signal Blue/Yellow
FPR Fuel pump relay output Blue/Red
W Warning/check light output Green/White
STP Brake light input Green/White
ABS ABS signal (optional) Green/White
FC Fuel cut ouput Green/Red
ELS Electricals idle up input Black
+B1 Permanent +12V Black/Yellow
+B Permanent +12V Black/Yellow
BAT Permanent +12V White/Red
