			2000 Pontiac Sunfire Alarm, Remote Start, Keyless Entry Wiring Information

	Constant 12V+
	Red 
	Ignition Switch Harness 

	Starter
	Yellow 
	Ignition Switch Harness 

	Ignition
	Pink 
	Ignition Switch Harness 

	Ignition 2
	White 
	Ignition Switch Harness PCM and Cluster 

	Accessory
	Orange 
	Ignition Switch Harness (Heat/AC) 

	Tach
	White 
	Harness near Battery 

	Neutral Safety Wire
	Yellow 
	Ignition Switch Harness 

	Brake Switch
	White 
	Brake Switch 

	Trunk Release
	Black/White (+) 
	OEM Keyless Module Driver's Side of Trunk 

	Trunk Pin
	Black (+) 
	Light in Trunk 

	Parking Lights
	Brown (+) 
	Light Switch 

	Head Lamp
	Dark Blue (-) 
	Pink (-) at Head Light Switch 

	Door Trigger
	Green/Black (-) 
	And LT. Blue Block near Brake Diode Isolate 

	Door Lock
	Light Blue 
	Either Kick Panel (Passenger's Switch is Master) 

	Door Unlock
	White 
	Reverse Polarity 

	Driver's Lock
	Gray 
	Driver's Kick Panel 

	Driver's Unlock
	Tan 
	Driver's Kick Panel 

	Horn Wire
	Black (-) 
	HEADLamp Switch 

	Windows Up
	LF=Dark Blue, RF=Light Blue, LR=Dark Green, RR=Light Green 

	Windows Down
	LF=Brown, RF=Tan, LR=Purple, RR=Purple 









